Group A – Electric Driven

|  |  |
| --- | --- |
| A1 Pedestrian | Pallet trucks; Stillage trucks: Low lift platform trucks; Low lift order pickers |
| A2 Rider | Pallet trucks; Stillage trucks: Low lift platform trucks; Low lift order pickers |
| A3 Pedestrian | Fork lift trucks |
| A4 Pedestrian | High lift platforms |
| A5 Pedestrian | Pallet stackers |
| A6 Pedestrian | Straddle trucks |
| A7 Pedestrian | Reach trucks |
| A8 Rider | Stand on Reach trucks |

Group B – Electric & I.C.E Driven

|  |  |
| --- | --- |
| B1 Rider | Counterbalance forklift truck up to 5000kgs |
| B2 Rider | Counterbalance forklift truck up to, and including 15000kgs |
| B3 Rider | Counterbalance forklift trucks over 15000kgs |

Group C – Electric & I.C.E Driven

|  |  |
| --- | --- |
| C1 Rider | Sideloader lift trucks up to and including 5000kgs |
| C2 Rider | Sideloader lift trucks up to and including 15000kgs |
| C3 Rider | Sideloader lift trucks over 15000kgs |

Group D – Electric Driven

|  |  |
| --- | --- |
| D1 Rider | Reach & Straddle trucks |
| D2 Rider | Pallet stackers |

Group E – Electric Driven

|  |  |
| --- | --- |
| E1 Rider | Medium lift order picker |
| E2 Rider | High lift order picker |

Group F – Electric Driven

|  |  |
| --- | --- |
| F1 Rider | Very Narrow Aisle lateral (& front) stacking trucks – Man Up |
| F2 Rider | Very Narrow Aisle lateral (& front) stacking truck – Man Down |

Group G – I.C.E Driven

|  |  |
| --- | --- |
| G1 Rider | Straddle carriers |
| G2 Rider | Counterbalance container handling trucks |
| G3 Rider | Sideloader container handling trucks |
| G4 Rider | Telescopic container handling trucks |

Group H – Electric & I.C.E Driven

|  |  |
| --- | --- |
| H1 Rider | Tow tractor & trailer |
| H2 Pedestrian | Tow tractor & trailer – Including flip-up platform |
| H3 Rider | Tow tractor & trailer – Over 30,000kg |

Group J – I.C.E Driven

|  |  |
| --- | --- |
| J1 Rider | Rough Terrain masted counterbalance lift truck |
| J2 Rider | Rough Terrain variable reach (telescopic) lift trucks up to 9m lift |
| J3 Rider | Rough Terrain variable reach (telescopic) lift trucks over 9m lift |
| J6 Rider | Rough Terrain variable reach lift (telescopic), rotating turrent under 9m lift, 2 or 4 wheel steer |
| J7 Rider | Rough Terrain variable reach lift (telescopic), rotating turrent over 9m lift, 2 or 4 wheel steer |

Group J – I.C.E Driven

|  |  |
| --- | --- |
| J4 Rider | Industrial variable reach lift (telescopic) trucks up to 9m lift, 2 or 4 wheel steer |
| J5 Rider | Industrial high reach lift (telescopic) trucks over 9m lift, 2 or 4 wheel steer |

Group M – Electric Driven

|  |  |
| --- | --- |
| M Rider | Bi & Multi directional lift trucks |

Group P – Electric Driven

|  |  |
| --- | --- |
| P Rider | Pivot Steer Trucks |

Group T – LC.E Driven

|  |  |
| --- | --- |
| T Rider | Transportable (vehicle mounted) lift trucks |

Group Z – Manual Operated

|  |  |
| --- | --- |
| Z1 Pedestrian | Pallet trucks |
| Z2 Pedestrian | Platform trucks |
| Z3 Pedestrian | Pallet stacker |
| Z4 Pedestrian | Straddle truck |